

# Upgrade Guide

## Upgrade through the system interface


1. Copy the upgrade firmware file to the U disk, and insert the U disk into the USB interface of the instrument
2. Open the “Update” in “UTILITY”, the system will pop up a menu to select the upgrade file



1. Select the corresponding upgrade file to enter the upgrade confirmation interface; click “Cancel” to cancel this upgrade, click “OK” to start the upgrade.




1. The system will first copy the upgrade package, prompting that the copy is complete and you can remove the U disk
2. After the upgrade is successful, restart the oscilloscope, and check the version number through the system information in UTILITY to confirm whether the upgrade is successful



## Upgrade via dedicated upgrade channel

1. Copy the upgrade firmware file to the U disk, and insert the U disk into the USB interface of the instrument
2. Restart the instrument, the system detects that there is an upgrade firmware in the U disk, and automatically enters the upgrade interface



1. According to the prompt, select the corresponding upgrade firmware and click Upgrade
2. The system will first copy the upgrade package, prompting that the copy is complete and you can remove the U disk
3. After the upgrade is successful, restart the oscilloscope, and check the version number through the system information in UTILITY to confirm whether the upgrade is successful

