
# Firmware Upgrade Guide


**Note: The upgrade file software version must be higher than or equal to the current oscilloscope software version.**

[Warning] Please do not disconnect the power during the upgrade process!

1. Copy the upgrade file of the corresponding model into a USB flash disk and insert the USB flash disk into the USB port of the instrument.
2. Reboot the instrument and enter the upgrade interface, select the upgrade file by rotating the multi-function knob and press the multi-function knob to enter the upgrade process.



1. When prompted to upgrade successfully, remove the USB flash drive and reboot the computer.



1. If the upgrade fails, please check whether the firmware corresponds to the current version.
2. After reboot, check the model number and version number through UTILITY→System Information to confirm whether the upgrade is successful.