
# UPO1000 firmware upgrade guide


**Note: The software version of the upgrade file must be greater than or equal to the current oscilloscope software version.**

[Warning] Do not cut off the power during the upgrade process!

1. Copy the upgrade file "SysUpdate1000X" of the corresponding model to a USB flash drive, and insert the USB flash drive into the instrument's USB interface.
2. Restart the instrument, enter the upgrade interface, select the upgrade file by rotating the multi-function knob, and press the multi-function knob to enter the upgrade process.



1. If the upgrade is successful, remove the USB flash drive and restart the computer.



1. If it prompts that the upgrade failed, please check whether the firmware corresponds to the current version.
2. After restarting, use UTILITY → System Information to check the model number and version number to confirm whether the upgrade was successful.