
# Upgrade Guide

1. Decompress the zip archive of the corresponding model.
2. Copy the decompressed upgrade firmware file SysUpdate to the U disk, and insert the U disk into the USB port of the instrument.
3. Restart the instrument, enter the upgrade interface, and automatically upgrade.



1. When the screen prompts that the upgrade is successful, remove the USB flash drive and reboot.
2. If it prompts that the upgrade fails, please check whether the firmware corresponds to the current version.
3. After restarting, check the model and version number through UTILITY→System Information to confirm whether the upgrade is successful.

