

# Upgrade Guide

## Upgrade through the system interface


1. Check the current hardware version of UTG9000T. Download the corresponding version firmware from the official website.




1. Save the firmware to be upgraded in the root directory of the U disk



1. Insert the U disk into the USB interface of UTG9000T. The instrument will recognize the U disk and pop up a pop-up box "Upgrade file detected，upgrade now?". Click "OK" to confirm and start the upgrade.



1. Wait for the upgrade progress to complete, and the instrument will automatically restart without intervention.



1. After the instrument restarts, unplug the USB flash drive. Enter the system information page to view the current version information.

