
# Upgrade Guide

## Upgrade through the system interface

1. Check the current hardware version of UTG9000T. Download the corresponding version firmware from the official website.



1. Save **ALL** firmware files to be upgraded in the root directory of the U disk.
2. Insert the U disk into the USB interface of UTG9000T. The instrument will recognize the U disk and pop up a pop-up box "Upgrade file detected，upgrade now?”

A screen shot of a computer


AI-generated content may be incorrect.

1. Select file to be upgraded by touching screen to highlight blue, then touch "OK" on screen to confirm and start the upgrade.

A screen shot of a computer

AI-generated content may be incorrect.

1. Wait for the upgrade progress to complete, and the instrument will automatically restart without intervention.



1. After the instrument restarts, unplug the USB flash drive. Enter the system information page to view the current version information.

