
# Firmware Upgrade Guide

**Upgrade through the system interface**

1、Check the current hardware version of the machine. Download the appropriate version of firmware from the official website.

System or tap the settings button under the display area.



2、Save the firmware to a USB flash drive.


图形用户界面, 文本, 应用程序, 电子邮件

描述已自动生成

3、Insert the USB flash drive into the front USB port of the panel, touch and click the Folder button 图片包含 文本


描述已自动生成 in the display area, enter the file system, then touch the upper left corner of the Select the inserted USB flash drive device, and then select the folder where the firmware is stored, double-click  or click the "Load" in the right menu, you will enter the interface of whether or not to upgrade the prompts: the upgrade will overwrite the existing program, Are you sure to do so? Click below 电脑屏幕的照片

中度可信度描述已自动生成 to confirm the upgrade.



Click

double-click



4、Wait for the upgrade to complete and the instrument will automatically reboot without intervention, a normal reboot will complete the upgrade.

5、After the instrument reboots, unplug the USB flash drive. Go to the System Information page to view the current version information.

屏幕的截图

描述已自动生成