
**UDP3000S DC power supply firmware upgrade guide**

* Select the upgrade file according to the model and put it in the root directory of the FAT32 format U disk (the file name cannot be modified).
* Insert the USB flash drive into the machine to be upgraded then power off.

Note: Use USB port at back of machine. Not front USB port.

* Press and hold the "UTILITY" button and hit power button to turn on the power supply and start the upgrade.



* After the upgrade is completed, Remove USB and manually restart the machine, by hitting power button.



**Language change procedure**.

* If after upgrade the unit defaults to Chinese. Follow this procedure.



* Press “Utility” button
* Use knob and rotate to Setup. (4th menu down)
* Use knob and rotate to desired language: Chinese, English, Deutsch